#!/bin/bash
qjackctl -s -p Onboard48K &
echo "Waiting 4sec to let JACK start."
sleep 4.0s
jack-rack -s bass /home/music/projects/music-production/jack-rack-presets/onboard/yamaha-trb &
#jack-rack -s mix /home/music/projects/music-production/jack-rack-presets/M48-Mix &
#jack-rack -s mix_drums /home/music/projects/music-production/jack-rack-presets/M48-Mix-Drums &
jack-rack -s headphones /home/music/projects/music-production/jack-rack-presets/onboard/headphones &
